


**Kwin Map Prepartaion**


1. **Export Shp file from Geomedia file, (there are 9 files output and used (plotno shp only for matching)) these many data are exported by manually**




****


**After that Add field name as “ Kwin No “ in “K\_601A\_\_plotno.shp” file and write the name of the current file within each attribute table**

****


1. **Export AutoCad file of Myanmarannnotaion from Geomedia**

****

1. **Run Python script to change format of many AutoCAD file annotation to shape file to join with parcel kwin**

****

**The flollwing picture is the result of script anootation to shp conversion**

****


**Merging annotation shape point with python**

****

**Spatial join with kwin parcel (polygon) shp file and annotation shp (point)**

**Join option (Join\_one\_to\_one)**

**Match optin (Contains)**

****